BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x2C
Error In E2Data Found By E2Test

Default definition: |  | ALARM + EXTERN + ACTIVE |
Used by block: |  | E2 |
Category: |  | MAINTENANCE |

Some error in the E2 data structure was found by the E2 handler during internal tests, started by the supervision programs.

- D1: Test number

- 01h: Verify the RAM copy of the installed E2-maps. The error is always corrected.
- 02h: Search for base records with identical identity.
- 03h: Search for base records with identical directory number.
- 04h: Verify base record counter.
- 05h: Search for linked records with non-matching base record ID.
- 06h: Search for record pointers to non-installed maps.
- 07h: Search for record pointers to non-valid buffers.
- 08h: Search for record pointers to non-seized buffers.
- 09h: Search for seized buffers, which are not properly linked.
- 0Ah: Search for linked records with identical identity.
- 0Bh: Verify checksum of all installed maps.

- D2: Number of errors found in this test
- D3: Undefined
- D4: Undefined

#### Recommended action

This test can be repeated manually from BMS (Start RAM Test) without the generation of warnings. However, subtest number 1 repairs found errors, so these errors will normally not appear again. Use the button ‘REPAIR’ in BMS to repair the errors. NOTE: The repair function is normally executed by removing memory areas and the risk exists that certain functions can be lost. If the repair fails, replace the CPU-board and perform a cold start of the system. The system must then be reconfigured, either manually or from a back-up, if one exists.

Revision: PH2 © Ericsson Enterprise 2003