BusinessPhone Communication Platform 5.1
Commands > Commands 8000...8999

## 8405
Detecting carrier access codes

This command allows to specify the carrier access codes and its corresponding public (PTT) number. Up to 16 different access codes can be specified. Each access code and public number can have up to 10 digits.

The access code is the number which has to be dialled to get access to the carrier.

Example:

A carrier offers only international destinations. All international destination numbers start with 00. The external access code to be used to get access to the carrier network is specified as 190. The carrier has further specified that the two leading digits (00) need not be dialled.

Access code |  | Public Number |
190 |  | 00 |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003