BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2176
Gatekeeper zone definition

This command defines up to 6 IP-zones which contain a range of IP-addresses from which the Gatekeeper accepts registration requests.

##### Valid data

|  | low value |  | high value |
Zone1-6 |  | 0.0.0.0 -255.255.255.255 |  | 0.0.0.0 -255.255.255.255 |
Zone1-6 (default) |  | 0.0.0.0 |  | 0.0.0.0 |

Note

In case the default entries will not be modified, there is no zone definition which means all IP addresses will be accepted. If there is at least one zone definition, any other undefined zone will be ignored.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003