BusinessPhone Communication Platform 5.1
Commands > Commands 0000...0999

## 0143
Line break time for ELU-A

Line break time for analog extension.

With this command you can state the duration of a line break for an analog extension.

##### Valid data: 0 (default)-255 ms

The value zero indicates no line break.

The duration of a linebreak can vary from 1 * 50 ms to 255 * 50 ms.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD6 © Ericsson Enterprise 2003