BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1411
Time supervision for first digit at automatic incoming traffic

The command is used to state the supervision time for incoming calls between seizure and first digit. The parameter shall only be used for direct in-dialing lines and automatic incoming tie lines.

Value 0-255 seconds. Value = 0 means that no time supervision takes place.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003