BusinessPhone Communication Platform 5.1
Facilities

## Clock And Diary

## Definition

The system contains a realtime clock that is used to state the time and date of various functions in the system.

## Use

The clock in the system is used for the following functions:

- Reading of time and date on telephones with display
- To state time for CIL-(Call Information Logging) function
- Wake up in hotel system
- To block room-to-room traffic in hotel system at preprogrammed times
- For reminder facility, that is to call extension at programmed time
- Stamp sent messages with time and date that can be read off later
- Stamp alarms in the alarm centre function

## Operation

### STANDARD- and EXECUTIVE Telephones

Date and time are shown on the top row of the STANDARD - and EXECUTIVE telephones’ display.

The time can be displayed in the 24- or 12-hour mode.

#### 24 hour mode

The display shows e.g.: “10 Jul 14:40”

#### 12 hour mode

The display shows e.g.: “10 Jul 02:40 PM”

## Capacity

The time can be displayed in both the 24- and 12-hour modes. The diary takes into consideration the different number of days per month as well as leap years.

## Limitations

The clock has battery backup and can withstand loss of power for up to 200 hours.

## Programming

### Programming via the Telephone

6101 |  | Set year month day

Enter:

YY |  | year |  | (00-99) |
MM |  | month |  | (01-12) |
DD |  | day |  | (01-31) |

6103 |  | Set hour minute second

Enter:

HH |  | hour |  | (00-23) |
MM |  | minute |  | (00-59) |
SS |  | second |  | (00-59) |

6104 |  | 12h mode, display

For 12-hour mode the time is stated with AM and PM.

Default data: N = 24-hour mode.

### Programming via BMS

Time and date of ASB 150 02 can be set via BMS.

The command “set clock” is stated in the menu “system/system parameter”.

## Equipment

None

Revision: D © Ericsson Enterprise 2003