BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1940
UUS services activation request

This command states which UUS (User-to-User Signalling) services are subscribed and shall be requested at this interface.

Valid data:

- UUS not requested.
- UUS service 1 activation request
- UUS services 1 and 2 activation request
- UUS services 1 and 3 activation request
- UUS services 1, 2 and 3 activation request

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003