BusinessPhone Communication Platform 5.1
Commands > Commands 9000...9999

## 9140
4-th route choice

When all trunks in the 1-st route choice are busy, the call can be sent via another route. An alternative route shall be defined for the call to be rerouted.

Three different alternative routes can be defined.

- The 2-nd route choice is defined with command 9120 2nd-route choice
- The 3-nd route choice is defined with command 9130 3-rd route choice
- The 4-nd route choice is defined with command 9140 4-th route choice

The route directory number for the alternative route must exist before the command 91.. is programmed.

Valid values: 0-4 digits

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003