BusinessPhone Communication Platform 5.1
Commands > Commands 8000...8999

## 8021
RTR/DID time status

This command defines the usage of the status of the barring (8002 Room to room bar) and the open (8003 Room to room open) time:

Possible values:

1...times are valid for RTR and DID

2...times are valid for RTR only

3...times are valid for DID only

Initial value: 1

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003