BusinessPhone Communication Platform 5.1
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 7E SURDY

00h SUWARM |  | Warm start (normal restart) |
01h SUCOLD |  | Cold start (new e2base records) |
02h SUBLKRDY |  | Block ready (answer-message) |
03h SUALLRDY |  | All block ready for traffic |
04h SUBLKWAIT |  | Block needs more time for initialization |

Revision: PD2 © Ericsson Enterprise 2003