BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1038
Forward CLI/COL

This command is used to state, whether the received calling/connected number (CLI/COL) is to be forwarded in case of transit/gateway, or external diverted call.

Value =

0 Forward for transit/gateway calls, except to public net

1 Forward for transit/gateway calls

2 Forward for transit/gateway calls and external diverted calls

Intial value = 0

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003