BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x08
Transmission Level Adjust Failure

Default definition: |  | ERROR |
Default limit: |  | 65000 |
Used by block: |  | SX |
Category: |  | MAINTENANCE |

The level, requested by programming, was impossible to achieve. The range of transmission levels, possible to achieve, is not constant, but varies with the selected line impedance. When the requested level cannot be set, a level as close as possible is set instead and the warning counter is incremented.

- D1: Board position: 00h-3Fh
- D2: Individual number
- D3: Used relative send level (see message TRANSM, TRMNAK)
- D4: Used relative receive level (see message TRANSM, TRMNAK)

#### Recommended action

If the customer reports transmission level problems, the counter, associated with this warning, should be inspected. If the value is greater than zero, the counter limit should be set equal to zero. This action will generate this warning and next time the warning will be stored. The transmission level is determined by the commands for setting the nominal relative level (0140, 0141 and 1610, 1611) and by the commands for the selection and definition of transmission groups (0142, 1612 and 26xx).

Revision: PH2 © Ericsson Enterprise 2003