BusinessPhone Communication Platform 5.1
Commands > Commands 3000...3999

## 3706
ACD-I/O port for PC-graph

This command is used to state which line position is used for the communication channel. The stated line position shall be equipped with a board possessing a V.24-interface.

The line position is entered as: ppiii

where

pp = board position |  |

iii = individual of a V24 (IO Unit) port |  |

For programming of the line protocol see command group 60.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD4 © Ericsson Enterprise 2003