BusinessPhone Communication Platform 5.1
Commands > Commands 6000...6999

## 6407
CIL-data via CTI-link

This command enables the output of several bidirectional CIL formats via the serial interface of a CTI environment.

The CIL format is determined with command 6403 Format table.

If the format "Call CTI (out)" is chosen in command 6403 Format table or command 6407 CIL-data via CTI-link is set to YES, the line position of the CTI I/O port (command 8901 CTI port) is copied automatically to the position of the CIL I/O port (command 6401 Initiate I/O ports). In this case, changes of the line position of the CTI I/O port can only be performed by command 8901 CTI port.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2003