BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0xE3
RP IPU Warning

Default definition: |  | UNDEFINED |
Used by block: |  | IPU |
Category: |  | DESIGNER |

Lowest IPU warning level.

An abnormal condition in the program flow has been detected by the IPU software. The condition was safely handled by the software and does not require immediate user assistance.

- D1: Originating IPU software block, high byte
- D2: Originating IPU software block, low byte
- D3: Details on the fault reason, high byte
- D4: Details on the fault reason, low byte

Revision: PH2 © Ericsson Enterprise 2003