BusinessPhone Communication Platform 5.1
Commands > Commands 6000...6999

## 6014
Dialled number

The command determines the digits constituting the dialled number.

The following characters may be used:

0-9 Digit to be sent |  |

*,# Character to be sent |  |

- Wait for second dial tone |  |

Valid values: 20 digits

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2003