BusinessPhone Communication Platform 5.1
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 6C TONECTRL

0 TONE.STOP |  | Stop tone sending (reconnect last PCM) |
1 TONE.DIAL |  | Dial tone |
2 TONE.DIALSP |  | Special dial tone |
3 TONE.RINGSP |  | Special Ring Tone (internally to LINE 2) |
4 TONE.RING |  | Ring Tone (freq. used for call waiting) |
5 TONE.BUSY |  | Busy Tone |
6 TONE.CONG |  | Congestion Tone (blocked) |
7 TONE.NU |  | NU-tone |
8 TONE.ACK |  | Acknowledgement Tone |
9 TONE.CALLVP |  | Voice Paging Call Tone |
10 TONE.DISC |  | Disconnection Tone |
11 TONE.CALLHA |  | Hands-free Answering Call Tone |
12 TONE.ERRMIN |  | Minor Error Tone (Used by PR-block) |
13 TONE.ERRMAJ |  | Major Error Tone (Used by PR-block) |
14 TONE.QUEUE |  | Queue-tone |
15 TONE.INACT |  | Inactive tone |
16 TONE.CONF |  | Conference tone |
17 TONE.BI |  | Intrusion tone (Break in) |
18 TONE.BIOP |  | Intrusion tone (Break in from operator) |
19 TONE.CONFOP |  | Conference tone, operator |
20 TONE.PARK |  | Parking tone |
21 TONE.ALTRING |  | Alternative ring tone |
22 TONE.ALTBUSY |  | Alternative busy tone |
23 TONE.ALTNU |  | Alternative NU tone |
24 TONE.ALTDIAL |  | Alternative dial tone |
25 TONE.OKAY |  | Okay, continue (short muted tone burst) |
26 TONE.CWAIT |  | Call waiting (tone burst) |
27 TONE.CWAITR |  | Call waiting (repetitive) |
28 TONE.CONGRES |  | Congestion Tone (no resources) |
29 TONE.PUBDIAL |  | Public dial tone |
30 TONE.TEST |  | Test tone |
31 TONE.ERWT |  | Expensive Route Warning Tone |
1 TSCTONESTART |  | Start tone sending |
2 TSCTONESTOP |  | Stop tone sending |
3 TSCTONERDY |  | Tone sending stopped |
4 TSCTONEERROR |  | Illegal tone ordered |
5 TSCKSCSTART |  | Start digit sending |
6 TSCKSCSTOP |  | Stop digit sending |
7 TSCKSCRDY |  | Digit sending stopped |
8 TSCKSCERROR |  | Illegal DTMF ordered |
9 TSCSXREQUEST |  | Request of tone individual |
10 TSCSXSTART |  | Start/restart tone sending |
11 TSCSXRELEASE |  | Release of tone individual |
12 TSCSXACK |  | Okay |
13 TSCSXNAK |  | Not okay |

Revision: PD2 © Ericsson Enterprise 2003