BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2222
Number Serial Range

This command is used to define received external numbers which are relevant for an automatic incoming call (and are allowed to be handled).

Relevant numbers can be defined in number series as:

- The two most significant numbers for the min. number series and the two most significant numbers for the max. number series (e.g. 12-34).
- Only one number series is defined with the two most significant digits (e.g. 12).
- If no number series is programmed, all numbers are relevant.

Value: Max. 10 2-digit number series.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003