BusinessPhone Communication Platform 5.1
Dialogs

## Optimal Media Packet Size Table

This dialog shows the codec priority and the size for each codec in milliseconds. In order to avoid speech delay variation or conversation interruption (due to packet loss) the traffic situation on the LAN segment used for the VoIP lines should be analyzed. Depending on the selected voice transmission quality, a certain bandwidth will be occupied per voice call.

To access the dialog, open the “System” menu in the Configuration directory tree. Then open the “System parameters” submenu and click on “General IP data” to open the context menu. Now select “Media packet size” from the context menu.

For more information, click on the command link:

2169 |  | Optimal media packet size table

Actions

Submit |  | To submit your changes to the system. |
Reload |  | To reload the current system settings. |

For details please refer to Facility description - Networking via Voice over IP lines (366/155-34 ASB 150 02)

Revision: B © Ericsson Enterprise 2003