BusinessPhone Communication Platform 5.1
Commands > Commands 7000...7999

## 7436
Active alarm attempts

This command determines the number of times alarm messages may be sent in situations where the receiving device does not respond. Value 0-5.

‘Active alarm’ is a function which transfers alarms to an external alarm receiver.

Commands 7420 Service area id, 7421 Identity of exchange and 7430 Active alarm on?-7437 Max active alarms per day concern active alarms.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003