BusinessPhone Communication Platform 5.1
Commands > Commands 3000...3999

## 3701
Period initiation

The ACD-function includes routines for calculation of traffic statistics. It is necessary to define a measurement period so that calculation can take place. This command is used to state the time period for traffic statistics. The measurement period will be activated only if start time is set at a later time than the current time.

The start time should be defined as: ddhhmm

where |  |

dd = 00-31 (day) |  |

hh = 00-23 (hour) |  |

mm = 00-59 (minute) |  |

Minimum required authority level from telephone: 1

Accessible via BMS: No

Revision: PD4 © Ericsson Enterprise 2003