BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2601
Tone fragment definition

This command defines the tone fragments. A tone fragment consists of one or two frequencies and levels. The tone fragments are used as building element for the definition of traffic tones. See command 2620 Dial tone-2647 Congestion tone (resources). The number of tone fragments depends on the number of DTMF-signals (command 2610 Number of DTMF tones). If 12 DTMF-signals are defined, the number of tone fragments is 19, and if 16 DTMF signals are defined, the number of tone fragments is 15. Tone fragment number 0 is always silent.

Level: -64.0-+3.0 dBm0 in steps of 0.5 dBm0 |  |

Frequency: 300-3400 Hz |  |

If no tone fragment has been defined, level and frequency are presented as “-”.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003