BusinessPhone Communication Platform 5.1
Commands > Commands 0000...0999

## 0125
Voice mail extension?

This command is used to specify whether a voice-mail equipment is connected to an extension position or not. Only analogue extensions are possible.

A “normal” extension will receive tones according to the selected tonescheme while a voice-mail extension will receive tones adapted to this type of equipment.

##### Valid data: Yes / No (default)

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD6 © Ericsson Enterprise 2003