BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x7C
RP Resource Limit Nearly Exceeded

Default definition: |  | ERROR |
Used by block: |  | BTU, ELU-A |
Category: |  | DESIGNER |

The warning is sent, when only four of the limited resources of either buffers, timers or digit-storage is available.

- D1: Individual number or 0
- D2: Type of resources

- 00h: receive buffer limit
- 01h: External send buffer limit
- 02h: Internal buffer limit
- 03h: Timer limit
- 04h: Digit position limit

- D3: Undefined
- D4: Undefined

Revision: PH2 © Ericsson Enterprise 2003