BusinessPhone Communication Platform 5.1
Commands > Commands 9000...9999

## 9103
NPI for private calling/connected line identification

The command is used to define the Number Plan Identifier (Number Plan and Type Of Number) for private calling/connected line and name identification.

Following combinations of NP’s and TON’s are available for the CN calls:

NP/TON | PRIVATE NP (QSIG) | UNKNOWN NP (QSIG)
| Regional level 1, PNP/RL1 (regional) | Unknown
| Regional level 0, PNP/RL0 (local) |
| Unknown, PNP/UNK |

Value:

PNP/UNK

PNP/RL0

PNP/RL1

UNK/UNK

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003