BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2008
Verification tone on call back

The system supplies normal verification tone when it accepts an order. This can be altered so that silence is received instead.

valid data: YES (verification tone), NO (silence)

default data: YES

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003