BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2260
DDI/CN number translation

The number translation tables, ‘DDI1’ and ‘DDI2’, allow programming of two separate number translations for up to 400 internal directory numbers in up to 200 intervals.

Each trunk can be programmed (command 1804 DDI number translation) with a number reference value to one or both of these translation tables. The contents of these tables are used for the translation of external DDI/CN numbers to corresponding internal directory numbers and vice versa.

The system command 2263 Type of individual number translation makes it possible to enable the usage of DDI numbers also for internal calls according to one, or both translation tables of the “Individual number translation table”.

If an external or internal number is not found in the tables, no translation can be done, and the ordinary number analysis will be performed for the received external DDI/CN number and the internal dir. number is used for the calling/connected identification services.

Table syntax

- ‘Internal directory number’ =
  1-4 digit internal directory number

- the number must be defined in the system
- a number interval is defined by separating two directory numbers with a comma (e.g. 200,209)

- ‘DDI1 no’, ‘DDI2 no’ =
  1-8 digit external (DDI/CN) number used in the public and/or private number plan

- for a number interval only the first number has to be entered (e.g. 4000)

##### Valid data

Int. Dir.No |  | valid internal number directory range ( default =empty) |
DDI 1 |  | 1-8 digits (0 - 9, *, #) |
DDI 2 |  | 1-8 digits (0 - 9, *, #) |

##### Examples of how to create a number translation

number range |  | DDI no.1 |  | DDI no.2 |
0 |  | 300 - 309 |  |  |
1 |  | 812 - 841 |  |  |
2 |  | *800 - *809 |  | *9000000 - *9000009 |
3 (3300 - 3399) |  | 600 - 699 |  | 6900 - 6999 |
4 (4440 - 4449) |  | 700 - 799 |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003