BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1942
UU-information length for UUS service 1

This command states which maximal UUI (User-to-User Information) length in UUS (User-toUser Signalling) service 1 is supported at this interface.

Valid data:

0: 128 octets

1: 32 octets

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003