BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x77
CARD TYPE WARNING.

Default definition: |  | ERROR |
Used by block: |  | BTU-B, BTU-DP, MFU |
Category: |  | DESIGNER |

This warning represents a warning code for the ISDN interface boards and also the MFU board. The warning is used as help for the responsible designer.

Check the board position to define the card type.

- D1: Function ID
- D2: Warning type
- D3: User-defined data
- D4: User-defined data

Revision: PH2 © Ericsson Enterprise 2003