BusinessPhone Communication Platform 5.1
Commands > Commands 4000...4999

## 4315
Silent detect level VMU-HD

The detection of silence is implemented on the VMU-HD board. When silence is detected during recording of a voice message the central software will be informed and can take appropriate action.

This command defines the silence detection level. Values below are regarded as silence.

Valid values are -70 dBm--20 dBm.

Default value is -40 dBm

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003