BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1005
Common abbreviated number COS

The command states to which abbreviated number category the trunk belongs.

The abbreviated number category determines which common abbreviated numbers are open for the trunk.

Trunks (and extensions) can be divided into four different abbreviated number categories (value 0-3).

For each common abbreviated number it is possible to determine which category or categories shall be open for the abbreviated number.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003