BusinessPhone Communication Platform 5.1
Facility Description – General

## Function of ASB 150 02 With/Without Connected FECU

Together with the introduction of the ASB 150 02 Release 9, the software licensing concept was introduced.

Most of the features, that were introduced from the Software Release ASB 150 02 Release 9 and upwards can only be enabled by a FECU, which is connected to the CPU-D4.
Each major commercial release (e.g. BusinessPhone Version 3, Version 4, Version 5 ...) has its own FECU series, covering several packages.

#### BusinessPhone Communication Platform - Version 3 (ASB 150 02 R9 / R10)

FECU article number: KDUBS 130 06 / x
(x = Package 1-10)

Package 1: |  | Basic Functions R9 / R10

Package 2: |  | Standard digital networking with max. 32 trunk interfaces

Package 3: |  | Standard digital networking with unlimited trunk interfaces

Package 4: |  | Full digital networking with max. 32 trunk interfaces

Package 5: |  | Full digital networking with unlimited trunk interfaces

Package 6: |  | CTI

Package 7: |  | CTI+ Standard digital networking with max. 32 trunk interfaces

Package 8: |  | CTI + Standard digital networking with unlimited trunk interfaces

Package 9: |  | CTI + Full digital networking with max. 32 trunk interfaces

Package 10: |  | CTI + Full digital networking with unlimited trunk interfaces

#### BusinessPhone Communication Platform - Version 4 (ASB 150 02 R11)

FECU article number: KDUBS 130 07 / x
(x = Package 1-10)

Package 1: |  | Basic Functions R11

Package 2: |  | Standard digital networking with 32 trunk interfaces

Package 3: |  | Standard digital networking with unlimited trunk interfaces

Package 4: |  | Full digital networking with 32 trunk interfaces

Package 5: |  | Full digital networking with unlimited trunk interfaces

Package 6: |  | CTI + Full digital networking with 4 trunk interfaces

Package 7: |  | CTI + Standard digital networking with 32 trunk interfaces

Package 8: |  | CTI + Standard digital networking with unlimited trunk interfaces

Package 9: |  | CTI + Full digital networking with 32 trunk interfaces

Package 10: |  | CTI + Full digital networking with unlimited trunk interfaces

#### BusinessPhone Communication Platform - Version 5.0 (ASB 150 02 R12)

FECU article number: KDUBS 130 12 / x
(x = Package 1-10)

Package 1: |  | Basic Functions R12+ Full digital networking with 2 trunk interfaces

Package 2: |  | Standard digital networking with 32 trunk interfaces

Package 3: |  | Standard digital networking with unlimited trunk interfaces

Package 4: |  | Full digital networking with 32 trunk interfaces

Package 5: |  | Full digital networking with unlimited trunk interfaces

Package 6: |  | CTI + Full digital networking with 4 trunk interfaces

Package 7: |  | CTI + Standard digital networking with 32 trunk interfaces

Package 8: |  | CTI + Standard digital networking with unlimited trunk interfaces

Package 9: |  | CTI + Full digital networking with 32 trunk interfaces

Package 10: |  | CTI + Full digital networking with unlimited trunk interfaces

#### BusinessPhone Communication Platform - Version 5.1 (ASB 150 02 R13)

FECU article number: KDUBS 130 13 / x
(x = Package 1-10)

Package 1: |  | Basic Functions R13+ Full digital networking with 2 trunk interfaces

Package 2: |  | Standard digital networking with 32 trunk interfaces

Package 3: |  | Standard digital networking with unlimited trunk interfaces

Package 4: |  | Full digital networking with 32 trunk interfaces

Package 5: |  | Full digital networking with unlimited trunk interfaces

Package 6: |  | CTI + Full digital networking with 4 trunk interfaces

Package 7: |  | CTI + Standard digital networking with 32 trunk interfaces

Package 8: |  | CTI + Standard digital networking with unlimited trunk interfaces

Package 9: |  | CTI + Full digital networking with 32 trunk interfaces

Package 10: |  | CTI + Full digital networking with unlimited trunk interfaces

The term “trunk interface” in the table above, has the meaning of one (1) connection used for private network communication. It corresponds hence to one (1) B-channel of the BA or PRA or (1) voice channel on the IPU, which is used for private network traffic.

Features which were introduced in a Release earlier than ASB 150 02 R9 are always enabled, and therefore also accessible if no FECU is connected to the CPU-D4. Furthermore fault corrections to existing unprotected features, as well as small feature improvements are always enabled.
Only two features are excluded from this philosophy: These are the "BusinessLink for Novell" and "proprietary CTI Interface", which were introduced in ASB 150 02 R8. To run the "BusinessLink for Novell" and "proprietary CTI Interface" on the system with R9 Software or upwards, the related FECU (see following table) is required.

The Package 1 always represents the new basic functionality of the Release, which is of course also included in all packages with a higher index.
If you upgrade a system to a higher SW-Release, without changing the FECU although the new Release has its own FECU series (separate article number), the system will remain on the same feature level, except for those features that are not protected.

#### Functionality enabled in ASB 150 02 depending on the connected FECU

- KDUBS 130 06 / 1-10 (ASB 150 02 R9, R10)
- KDUBS 130 07 / 1-10 (ASB 150 02 R11)
- KDUBS 130 12 / 1-10 (ASB 150 02 R12)
- KDUBS 130 13 / 1-10 (ASB 150 02 R13)

The entries in the table indicate the minimum FECU version (last two digits of the article code), for the respective feature. The FECU version may not specifically be equal to the SW version the feature was introduced.

Feature | no FECU (not protected) | FECU KDUBS 130 xx/1 | FECU KDUBS 130 xx/2 | FECU KDUBS 130 xx/3 | FECU KDUBS 130 xx/4 | FECU KDUBS 130xx/5 | FECU KDUBS 130 xx/6 | FECU KDUBS 130 xx/7 | FECU KDUBS 130 xx/8 | FECU KDUBS 130 xx/9 | FECU KDUBS 130 xx/10
Abbreviated no. dial.- common numbers | X |  |  |  |  |  |  |  |  |  |
Abbreviated no. dial.- individual numbers via key pad |  | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06
Abbreviated no. dial.- individual numbers via prog. key | X |  |  |  |  |  |  |  |  |  |
Account numbers | X |  |  |  |  |  |  |  |  |  |
Account numbers (verified) |  | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13
ACD Group | X |  |  |  |  |  |  |  |  |  |
ACD Agent &Supervisor | X |  |  |  |  |  |  |  |  |  |
ACD - Multiple call codes |  | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06
ACD - Queue Exit |  | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13
Alarm function | X |  |  |  |  |  |  |  |  |  |
Authority code | X |  |  |  |  |  |  |  |  |  |
Automatic callback | X |  |  |  |  |  |  |  |  |  |
Automatic Redial |  | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13
Background music | X |  |  |  |  |  |  |  |  |  |
Automated Attendant | X |  |  |  |  |  |  |  |  |  |
Call metering | X |  |  |  |  |  |  |  |  |  |
Call metering - Austria |  | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07
Call p. up - common | X |  |  |  |  |  |  |  |  |  |
Call p. up - ext. group | X |  |  |  |  |  |  |  |  |  |
Call p. up - individual | X |  |  |  |  |  |  |  |  |  |
Call waiting indication | X |  |  |  |  |  |  |  |  |  |
Camp on | X |  |  |  |  |  |  |  |  |  |
Clock and diary | X |  |  |  |  |  |  |  |  |  |
Clock and diary (synchronisation with ISDN) |  | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13
Common bell | X |  |  |  |  |  |  |  |  |  |
Conference | X |  |  |  |  |  |  |  |  |  |
Conn. state mess. | X |  |  |  |  |  |  |  |  |  |
Conversation recording |  | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12
CTI - proprietary CTI Interf. * |  |  |  |  |  |  | 06 | 06 | 06 | 06 | 06
CTI - BusinessLink for Novell * |  |  |  |  |  |  | 06 | 06 | 06 | 06 | 06
CTI - BusinessLink for Windows NT |  |  |  |  |  |  | 06 | 06 | 06 | 06 | 06
CTI - BusinessLink for Win NT - only Support of OWS, AAO |  | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06
CTI groups =< 8 ** |  |  |  |  |  |  | 06 | 06 | 06 | 06 | 06
CTI groups =< 16 |  |  |  |  |  |  | 07 | 07 | 07 | 07 | 07
CTI - Enhanced CIL func. |  |  |  |  |  |  | 06 | 06 | 06 | 06 | 06
Dictaphone | X |  |  |  |  |  |  |  |  |  |
DISA | X |  |  |  |  |  |  |  |  |  |
Diversion direct | X |  |  |  |  |  |  |  |  |  |
Diversion individual (Follow me) | X |  |  |  |  |  |  |  |  |  |
Diversion on busy | X |  |  |  |  |  |  |  |  |  |
Div. on no reply | X |  |  |  |  |  |  |  |  |  |
Doorphone (answering) | X |  |  |  |  |  |  |  |  |  |
DTMF tones | X |  |  |  |  |  |  |  |  |  |
DTMF tones at inc. calls | X |  |  |  |  |  |  |  |  |  |
Fault indication | X |  |  |  |  |  |  |  |  |  |
Fax extension | X |  |  |  |  |  |  |  |  |  |
Fictive numbers (<16) | X |  |  |  |  |  |  |  |  |  |
Fictive numbers (<1000) |  | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07
Group hunting (PBX-Group) with serial distribution | X |  |  |  |  |  |  |  |  |  |
Group hunting (PBX-Group) with parallel distribution |  | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07
Hot line | X |  |  |  |  |  |  |  |  |  |
Hotel facilities | X |  |  |  |  |  |  |  |  |  |
Immediate answer | X |  |  |  |  |  |  |  |  |  |
Individual external diversion |  | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12
Individual number translation external |  | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07
Individual number translation internal |  | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13
Information via Info-key | X |  |  |  |  |  |  |  |  |  |
Information via keypad |  | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06
Inquiry | X |  |  |  |  |  |  |  |  |  |
Integrated Cordless - A protocol | X |  |  |  |  |  |  |  |  |  |
Integrated Cordless - GAP 1.0 protocol |  | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06
Integrated Cordless - GAP 2.0 protocol |  | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12
Intercom | X |  |  |  |  |  |  |  |  |  |
Intrusion | X |  |  |  |  |  |  |  |  |  |
IP Extension |  | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13
ISDN BA & PRA | X |  |  |  |  |  |  |  |  |  |
ISDN S-interface | X |  |  |  |  |  |  |  |  |  |
ISDN Caller List |  | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06
ISDN Call forwarding with partial rerouting |  | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13
ISDN DDI, AOC | X |  |  |  |  |  |  |  |  |  |
ISDN CLIP, COLP | X |  |  |  |  |  |  |  |  |  |
ISDN CLIR, COLR | X |  |  |  |  |  |  |  |  |  |
ISDN - CLIR override |  | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06
ISDN MCID, MSN, SUB | X |  |  |  |  |  |  |  |  |  |
ISDN - Point to MultiPoint |  | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07
Key system function | X |  |  |  |  |  |  |  |  |  |
Last ext.numb.redial | X |  |  |  |  |  |  |  |  |  |
Least Cost Routing | X |  |  |  |  |  |  |  |  |  |
Line signal schemes | X |  |  |  |  |  |  |  |  |  |
Loudspeaker paging | X |  |  |  |  |  |  |  |  |  |
Mailbox-system | X |  |  |  |  |  |  |  |  |  |
Mailbox-system - individual greeting |  | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07
Mailbox-system - outcall notification |  | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13
Manipulation of metering costs |  | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07
Message-system voice | X |  |  |  |  |  |  |  |  |  |
Message-system call me | X |  |  |  |  |  |  |  |  |  |
Message-system text | X |  |  |  |  |  |  |  |  |  |
Music on hold - external (1 source) | X |  |  |  |  |  |  |  |  |  |
Music on hold- integrated (1 source) |  | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07
Music on hold (1 integrated and 7 external sources or 8 external sources) |  | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12
Name selection | X |  |  |  |  |  |  |  |  |  |
National spec.functions - Croatia: Adaptation of CN numbering plan |  | 12 | 06 | 06 | 06 | 06 | 07 |  |  | 06 | 06
National spec.functions - Spain: Ibercom Indicat. |  | 12 | 06 | 06 | 06 | 06 | 07 | 06 | 06 | 06 | 06
National spec.functions - Poland: Testcall | X |  |  |  |  |  |  |  |  |  |
National spec.functions - Austria: Support of packet mode terminals |  | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07
National spec.functions - Italy: ISDN three party conference |  | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13
National spec.functions - New Zealand: Centrex hook flash over ISDN |  | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13
Networking - based on analogue lines | X |  |  |  |  |  |  |  |  |  |
Networking - VPN service from PSTN | X |  |  |  |  |  |  |  |  |  |
Networking - based on digital/VoIP lines with QSIG (32 trunk interfaces) ***) |  |  | 06 | 06 | 06 | 06 |  | 06 | 06 | 06 | 06
Networking - based on digital/VoIP lines with QSIG (unlimited trunk interfaces) ***) |  |  |  | 06 |  | 06 |  |  | 06 |  | 06
Networking - based on digital/VoIP lines with QSIG+UUS (2 trunk interfaces) |  | 12 |  |  | 06 | 06 | 07 |  |  | 06 | 06
Networking - based on digital/VoIP lines with QSIG+UUS (4 trunk interfaces) |  |  |  |  | 06 | 06 | 07 |  |  | 06 | 06
Networking - based on digital/VoIP lines with QSIG+UUS (32 trunk interfaces) ***) |  |  |  |  | 06 | 06 |  |  |  | 06 | 06
Networking - based on digital/VoIP lines with QSIG+UUS (unlimited trunk interfaces) ***) |  |  |  |  |  | 06 |  |  |  |  | 06
Networking - based on digital/VoIP lines with UUS mapped into GFP |  | 12 |  |  | 07 | 07 | 07 |  |  | 07 | 07
Networking - based on digital/VoIP lines - Central. Operator #) |  | 12 |  |  | 07 | 07 | 07 |  |  | 07 | 07
Night service | X |  |  |  |  |  |  |  |  |  |
O&M - Swapping boards during operation |  | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06
O&M -Remote SW upgrading |  | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06
O&M -Remote FW upgrading |  | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12
O&M - Cordless remote programming |  | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06
Paging | X |  |  |  |  |  |  |  |  |  |
Park.for com.access | X |  |  |  |  |  |  |  |  |  |
Parking individual | X |  |  |  |  |  |  |  |  |  |
Private trunk line | X |  |  |  |  |  |  |  |  |  |
Programmable and fixed keys | X |  |  |  |  |  |  |  |  |  |
Refer back | X |  |  |  |  |  |  |  |  |  |
Register recall in PSTN | X |  |  |  |  |  |  |  |  |  |
Reminder service | X |  |  |  |  |  |  |  |  |  |
Saved ext. no. redial | X |  |  |  |  |  |  |  |  |  |
Secretary function | X |  |  |  |  |  |  |  |  |  |
Supervision | X |  |  |  |  |  |  |  |  |  |
Tandem - Slave | X |  |  |  |  |  |  |  |  |  |
Tandem - Master | X |  |  |  |  |  |  |  |  |  |
Telephone directory | X |  |  |  |  |  |  |  |  |  |
Voice Outcall Notification |  | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13
VoIP Interface (IPU) | X |  |  |  |  |  |  |  |  |  |
Testcall for Poland | X |  |  |  |  |  |  |  |  |  |
Trunk line key | X |  |  |  |  |  |  |  |  |  |
Voice mail box, external | X |  |  |  |  |  |  |  |  |  |

X * |  | Feature was introduced in a Release earlier than ASB 150 02 R9 The "proprietary CTI Interface" and "BusinessLink for Novell" were already released in ASB 150 02 R8 and are always enabled on the CPU-D3. In conjunction with the CPU-D4 a FECU device is required. |
** |  | This feature was previously called “CTI for Automated Attendant” |
*** |  | This capacity can not be reached only with VoIP lines, due to the fact that the IPU is limited to max. 8 voice channels |
#) |  | Following features are covered by the name COP - Supervision of busy with recall at free (similar to the Call Back on busy function) - Camp on - Intrusion with forced release - Recall at No Answer |

Revision: PC1 © Ericsson Enterprise 2003