BusinessPhone Communication Platform 5.1
Facilities

## ISDN SS Advice Of Charge (AOC)

## Definition

If this service is subscribed to at an outgoing call, currency or charging units are sent to the exchange, depending on the respective network operator. Three different types of how the currency or charging units are sent to the subscriber number are possible (depending on subscription and network operators provision).

#### AOC-D (Advice of Charge during the call)

At call setup to the public network, ASB 150 02 requests for continuous elapsed charging during the call and at the end of the call. This means that the already consumed charging information is always received during the call.

Users of STANDARD and EXECUTIVE telephones may read this charging information on their displays during the call.

#### AOC-E (Advice of Charge at the end of the call)

At call setup to the public network ASB 150 02 requests for the charging information to be provided at the end of the call. This means that after termination of the external call the recorded charging information is sent to the respective call meter of the extension.

#### AOC-permanently subscribed

Information on the recorded charges is automatically sent during and at the end of the call, without ASB 150 02 having to request this information from the public network.

## Use

The supplementary service AOC offers the possibility to get an overview of the recorded charges in the public network.

For further information see Call Metering (141/155 34-ASB 150 02 Uen).

## Operation

### System telephones

See Call Metering (141/155 34-ASB 150 02 Uen).

### ISDN terminals

See User’s Guide.

## Capacity

See Call Metering (141/155 34-ASB 150 02 Uen).

## Limitation

See Call Metering (141/155 34-ASB 150 02 Uen).

If an external call information logging system is connected to the ASB 150 02 and you receive only currency units from the public net, only the output format CIL2/CIL3 Hotel (command 6403) may be used. Only these formats contains additional fields for output of costs.

For further information see Format Description (9/155 19-ASB 150 02 Uen).

## Programming

1914 |  | Subscribed charging method

6710 |  | Currency identifier

6711 |  | Decimals in cost

6712 |  | Currency identifier last

8424 |  | Pulse cost metering

All further commands see Call Metering (141/155 34-ASB 150 02 Uen).

## Equipment

BTU-D with ISDN prom set or BTU-B_ or MFU.

Revision: K © Ericsson Enterprise 2003