BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1918
Provision of connected line identification

The command is used to define whether an ASB-party’s line directory number may be sent to the network.

The following ASB-number to network parameters are available:

NO: Connected ASB-party’s directory number not to network |  |

YES: Connected ASB-party’s directory number to network |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003