BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x45
VMU Reference Error

Default definition: |  | ERROR |
Used by block: |  | ALL |
Category: |  | DESIGNER |

A reference error in a message to a VMU has been detected by the VMU board. The error is indicated in the answer from the VMU board. Another possible reason for this warning is in case of no free VMU channel is available.

The warning is intended for the AN, IN and MG software blocks.

D1: | Error condition
| 01H ... | No free VMU channel available
| 02H - FFH ... | VMU reference error
D2: | Card position of VMU or MFU card
D3: | Undefined
D4: | Undefined

Revision: PH2 © Ericsson Enterprise 2003