BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1941
Explicit UUS service 1 activation request

This command states whether or not UUS (User-to-User Signalling) service 1 is requested explicitly at this interface.

Valid data:

NO: not requested (implicitly)

YES explicitly requested

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003