BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2024
Initiate public Dialtone at LCR

This command is used to state whether the public dialtone has to be sent to the caller, after dialling a directory number of a LCR-controlled trunk. The parameter programmed by this command is relevant only if command 2034 Initiate dial tone at LCR is set to YES.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003