BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2250
Destination Number Cross Reference Table

The Destination Number Cross Reference Table contains four columns which make possible to define destination numbers in four different directions. This table is only needed, if the PABX is connected via separate routes to networks with different number plans.

PREDIGITS |  | Specification of the predigits (up to 4 digits) defined for the trunks. |
DEST NO |  | The number of leading digits (up to 10 digits) of a destination number needed to identify the cost for a call. |
DEST NO GRP |  | The number of the group. It will be easier to get information allocating numbers from zero upwards to all groups that are created on the basis of official list prices of carriers and from 249 downwards to all groups created on the basis of special prices or e.g. tie lines. |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003