BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1420
Number of disconnection tone bursts

The command is used to state the number of tone bursts before a disconnection tone is accepted.

The duration of a tone burst is set with the commands 1421 Pulse time for disconnection tone burst, 1422 Pause time for disconnection tone burst.

Value = 0-10.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003