BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2160
Network connection (read only)

This command is used to read out if there is a physical connection to the LAN and if there is a established connection which type is used (equals to the LED indications on the IPU board)

Note

This command only functions in online mode

##### Valid data

0 |  | undefined (no connection established) |
1 |  | 10 BaseT |
2 |  | 100 BaseT |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003