BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1956
MSN provided to TEs?

This command states whether MSN (Multiple Subscriber Number) is provided by the terminal user(s) on the interface. If it is not provided,the called party number information is discarded and a global call is indicated to the interface.

Valid data:

No: MSN is not provided

Yes: MSN is provided

Note

This feature can only be used, if the ISDN-terminals are programmed also with the MSN number!

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003