BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2007
Rotary dial type

The command states the type of rotary dial telephone used in the system with respect to the number of pulses per digit.

value | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10
0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10
1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 1
2 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 10
3 | 10 | 9 | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003