BusinessPhone Communication Platform 5.1
Installation Instruction ASB 150 02 > Boards for ASB 150 02

## CPU-D2 (ROF 157 5118/2)
CPU-D3 (ROF 157 5118/3) AUX2 (ROF 1575 119/2) AUX3 (ROF 1575 119/3)

Before installing the board mount the system software PROMs in the appropriate positions.

#### Connections on the CPU-D2(3)/AUX2(3)

For connection of Temparture sensor kit, see chapter Temperature Sensor

The ALARM input is optically isolated and the voltage has to be between 20 - 60 VDC. The ALARM output is equipped with an open collector transistor with a capacity of 20 mA at 12 VDC (Maximum 14 VDC).

Revision: E © Ericsson Enterprise 2003