BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x90
OM Internal Error

Default definition: |  | ERROR |
Used by block: |  | OM |
Category: |  | DESIGNER |

This warning is used by the OM block to log errors that occur within the own block. The type of error is not considered to merit an unique error code.

- D1:
- D2: Type of error

- 01h: Invalid state.
- 03h: Invalid command number.
- 04h: Timeout.
- 05h: Error in byte OM.LSTCOD.
- 06h: E2NAK received.
- 07h: Data error in trace function.
- 08h: Error during INIT. No E2 data received.
- 09h: Unexpected data error.
- 0Ah: No INFO text found.
- 0Bh: No pointer to RAM in section MDATA found.
- 0Ch: Phase error during E2 status verification.
- 0Dh: No space left in SW protection table.
- 0Eh: No space left in resource check table.
- 0Fh: Error during BBRAM handling (OS.BATT).

- D3: Undefined
- D4: Undefined

Revision: PH2 © Ericsson Enterprise 2003