BusinessPhone Communication Platform 5.1
Dialogs

## Private Network Router -Parameters

Facilities of this type can be created, deleted, or altered using the standard facility management dialog.

To access the dialog, open the “Facilities” menu in the Configuration directory tree. Then open the “Networking” submenu and click on “Private Network Router”. The Edit/Change section shows all private network routers that have been created. Click on a Parameters link of a router to open the parameters dialog.

In the first section, you can set the directory number and name. The second section is called “General”. Here you can make the following settings:

9101 |  | Destination PBX

9102 |  | Call back allowed?

9103 |  | NPI for private calling/connected line identification

9104 |  | Call class

9105 |  | NPI for public calling/connected line identification

9110 |  | 1st-route choice

9111 |  | NPI for private/public called number

9112 |  | Remove digits choice 1

9113 |  | Predigits choice 1

9114 |  | Travelling Class Mark (TCM)

9115 |  | Complete called party NL

9116 |  | Subscriber called party NL

9117 |  | IP address reference

9120 |  | 2nd-route choice

9121 |  | NPI for private/public called number

9122 |  | Remove digits choice 2

9123 |  | Predigits choice 2

9124 |  | Travelling Class Mark (TCM)

9125 |  | Complete called party NL

9126 |  | Subscriber called party NL

9127 |  | IP address reference

9128 |  | Send expensive route warning tone

9130 |  | 3rd route choice

9131 |  | NPI for private/public called number

9132 |  | Remove digits choice 3

9133 |  | Predigits choice 3

9134 |  | Travelling Class Mark (TCM)

9135 |  | Complete called party NL

9136 |  | Subscriber called party NL

9137 |  | IP address reference

9138 |  | Send expensive route warning tone

9140 |  | 4th route choice

9141 |  | NPI for private/public called number

9142 |  | Remove digits choice 4

9143 |  | Predigits choice 4

9144 |  | Travelling Class Mark (TCM)

9145 |  | Complete called party NL

9146 |  | Subscriber called party NL

9147 |  | IP address reference

9148 |  | Send expensive route warning tone

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To reload the current system settings. |
Copy |  | To copy the current settings to another router. |
Back |  | To return to the previous dialog. |

See Facility Descriptions:

- Networking – Based On Analogue Lines
  (361/15534-ASB 150 02 Uen).
- Networking – VPN Service From PSTN
  (364/15534-ASB 150 02 Uen).
- Networking – Based On Digital Lines
  (365/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2003