BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x62
Trunk Line Without Call Metering

Default definition: |  | ERROR |
Used by block: |  | TR |
Category: |  | MAINTENANCE |

A line to the connected exchange has been used without a CM board on the trunk card, or the CM board did not answer.

- D1: Card position
- D2: Individual number
- D3: Undefined
- D4: Undefined

Revision: PH2 © Ericsson Enterprise 2003