BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1408
Minimum speech time for not increasing disturbance counter

The command is used to determine the minimum time a call shall have been established before disconnection.

Value 0-255 seconds

If disconnection takes place within the stipulated time the disturbance meter will be incremented.

The purpose of the disturbance meter is to identify trunks functioning poorly with regard to transmission quality, line faults, etc. When the disturbance meter reaches its maximum value the trunk will be disturbance-marked and thus can be no longer selected.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003