BusinessPhone Communication Platform 5.1
Commands > Commands 0000...0999

## 0158
Diversion on busy at external
calls ?

The command defines whether or not a diversion on busy on an external incoming call should be done.

If the extension is a master and a member of a tandem configuration the command data shall be copied to the slave and blocked for the slave's futher use.

##### Valid data: Yes /No (default)

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD6 © Ericsson Enterprise 2003