BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1316
Request A-number in MFC?

This command states whether the A-number shall be requested on incoming MFC signalling. This command does not affect the outgoing A-number transfer.

Valida data:

No: No request of A-number |  |

Yes: Request A-number |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003