BusinessPhone Communication Platform 5.1
Commands > Commands 3000...3999

## 3505
PBX queue overflow time

This command defines, how long a call will be queued in a PBX queue. After this time has been elapsed, the call will be rerouted to the exit position of the PBX group.

Valid data: 0 - 255 (seconds)

The value 0 will be interpreted as no queueing for the particular PBX group. A call, which arrives at a busy PBX group, will be rerouted immediately to the exit position of the PBX group. If no exit position has been defined, the default busy behaviour will take place.

Default data: 255

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD4 © Ericsson Enterprise 2003